FUNDUS IMAGE ANALYSIS AND GLAUCOMA RECOGNITION

A Project

Presented to the faculty of the Department of Computer Engineering California State University, Sacramento

Submitted in partial satisfaction of the requirements for the degree of

MASTER OF SCIENCE

in Computer Engineering

by

May-ku Nhiayi

FALL 2017

© 2017

May-ku Nhiayi

ALL RIGHTS RESERVED

ii

A Project by

May-ku Nhiayi

Approved by:

, Committee Chair Professor Fethi Belkhouche

, Second Reader Professor Warren D. Smith

Date

iii

Student: May-ku Nhiayi

I certify that this student has met the requirements for format contained in the University format manual, and that this project is suitable for shelving in the Library and credit is to be awarded for the project.

, Graduate Coordinator Professor Nik Faroughi Date

Department of Computer Engineering

iv

Abstract of

FUNDUS IMAGE ANALYSIS AND GLAUCOMA RECOGNITION

by

May-Ku Nhiayi

Glaucoma is a group of diseases that damage the eye’s optic nerve. If not treated, glaucoma can lead to vision loss or permanent blindness. Glaucoma is very problematic because often there are no symptoms in the early stages. Once symptoms appear, it could be too late to prevent blindness. There exist several methods to detect glaucoma such as tonometry, which examines the inner eye pressure, ophthalmoscopy, which examines the shape and color of the optic nerve, and perimetry, which tests for the complete field of vision. However, these methods do not allow to detect all types of glaucoma as the conditions vary from one person to another. Cup-to-disc ratio is a visual inspection method that can detect glaucoma. Image processing techniques such as binarization and superpixel classification are used in this project to calculate the cup-to-disc ratio and use it to determine if an eye has glaucoma.

Throughout the project, various details are needed for analyzing fundus images to detect glaucoma with image processing techniques. It is shown that the error margin is sensitive to many factors, including the color and quality of the image and the presence of

blood vessels. The results are not 100% accurate but with acquirement of better v

photographs and using more advanced technologies such as 3D imaging, the proposed methods can be improved in terms of the computation speed and accuracy.

, Committee Chair Professor Fethi Belkhouche

Date

vi

TABLE OF CONTENTS

Page List of Tables viii

List of Figures ix

Chapter

1. INTRODUCTION 1
2. PROPOSED ALGORITHM FOR GLAUCOMA DETECTION 4

[Glaucoma and its Characteristics 4](#_TOC_250005)

[Cup-to-disc Ratio 5](#_TOC_250004)

[Algorithm Steps 7](#_TOC_250003)

1. ANALYSIS OF THE DATA 11

[Healthy vs. Glaucoma Eyes 11](#_TOC_250002)

[Optic Disc Analysis 12](#_TOC_250001)

[Optic Cup Analysis 18](#_TOC_250000)

1. FINDINGS AND INTERPRETATIONS 24
2. SUMMARY AND CONCLUSIONS 33

Works Cited 36

vii

LIST OF TABLES

Tables Page

1. Glaucoma and healthy optic disc, optic cup sizes

(in pixels) and their ratio 25

viii

LIST OF FIGURES

Figures Page

1. Fluid pathway (in teal) in eye 4
2. Representation of cup-to-disc ratio 6
3. Fundus photograph 6
4. Optic disc (in yellow) and optic cup (in green) 7
5. Find optic cup process 9
6. Find optic disc process 10
7. Healthy eye 11
8. Glaucomatous eye 12
9. Red channel image from fundus photograph 13
10. Enhanced red channel from fundus photograph 14
11. Histogram of enhanced red channel 15
12. Binary image of fundus image using threshold 16
13. Regions detected by regionprop function 17
14. Optic disc region detected in red circle 17
15. Fundus image with optic disc on the left 18
16. Example with no distinct optic cup 19
17. Example of green and red channel histograms intercepting

before gray level index 100 20

1. Example of green and red channel histograms intercepting

after gray level index 100 21

ix

1. Image adjusted with imadjust function 22
2. Image segmented with superpixel function 22
3. Gray level superpixel image 23
4. Binary optic cup isolated 23
5. Optic cup area versus optic disc area 26
6. Glaucoma's fundus photograph with heavy blood vessels 27
7. Glaucoma's optic disc binary image with heavy blood vessels 28
8. Glaucoma's optic cup binary image with heavy blood vessels 29
9. Healthy fundus photograph with no defined optic cup 30
10. Binary image of healthy eye with no distinct cup 31
11. Healthy optic cup extraction - no defined optic cup case 31
12. 3D Fundus photograph 32

x

* 1. INTRODUCTION

Glaucoma, a set of eye diseases that can damage the optic nerve, is a leading cause of blindness. According to the Glaucoma Research Foundation [1], three million Americans have glaucoma, but only half of them know they have the illness. The Glaucoma Research Foundation lists several types of glaucoma, such as primary open-angle, angle- closure, and normal tension [2]. The National Eye Institute also defines glaucoma as a set of diseases that includes secondary, pigmentary, pseudoexfoliation and congenital glaucoma [3]. Glaucoma is not always easy to detect. As an example, acute angle-closure glaucoma does not show any physical symptoms or pain in the early stages [3]. Most people do not test for glaucoma on a regular basis. Therefore, many people with the disease are unaware of having it. An acute angle-closure attack, found in more advanced stages, would be the trigger for most people to test for the disease [3]. Pain from acute angle-closure attack can be relieved with medication or surgery; however, in secondary glaucoma, surgery is the only option [4]. Glaucoma is often called “the sneak thief of sight” [5]. If not detected in a timely manner; not only does it cause pain and steal one’s vision, but the medical bills are often very high. According to the Glaucoma Research Foundation’s facts and statistics, vision loss due to glaucoma diseases can never be reversed; however, the progression of the disease can be slowed down by medication or surgery [1]. It is crucial that glaucoma is detected as early as possible. Image processing techniques can be used to detect glaucoma in the early stages, which is crucial to preventing the disease from spreading and avoiding the potential pain and costs [6].

The use of image processing to detect glaucoma is not common in ophthalmic offices [7]. This approach consists of performing operations on an image in order to enhance it or isolate the desired information. The optic cup and disc ratio of an eye can determine whether a patient has glaucoma. The method consists of isolating the optic cup and disc and obtaining the ratio between them. The research paper *Superpixel Classification based Optic Cup Segmentation* [8] states that “the cup-to-disc ratio is a widely-used indicator for glaucoma” (page 1) in image processing, because the eye nerve fibers are gathered in this area, and when they are destroyed, the optic cup increases while the disc area remains the same. Evidence from Mishra Madhusudhan and fellow researchers’ paper suggests that glaucoma causes the interconnection between the photo receptors and the visual cortex to be reduced, which reduces the functional capabilities of the retina and changes the size of the cup [9]. Ophthalmoscopy is a current known method used by ophthalmologists to detect glaucoma. It consists of dilating the pupil to have a larger angle of view inside the eye; then the ophthalmologist examines the optic nerve using a magnifier, looking for any abnormalities, such as the shape and color of the optic nerve caused by glaucoma damage [7]. Image processing techniques could also be used to find the optic nerve’s shape and color since these visual aspects can be recorded and processed like the cup-to-disc ratio. This project however focuses on the cup-to-disc ratio. While it is possible to measure the area of the optic cup and disc manually, this method is subjective and prone to errors. Other tests such as tonometry that measures intraocular pressure, or the visual acuity test that measures how well a patient can see are subjective. The visual field test measures the peripheral vision; patients have to press a


button when they see the objects displayed by the machine to their peripheral view. Doctors also dilate the patient’s eye to examine the retina and the optic nerve [3]. These methods involve human interaction and interpretation, which can result in errors. Humans are more prone to making errors, which can be avoided by using more reliable and precise computer- based measurements. By using image processing techniques to obtain the cup-to-disc ratio, it will be easier to automate glaucoma detection and have more accurate data.

This project includes information about glaucoma and the application of image processing techniques for glaucoma detection. Our preliminary results show that these techniques can be more precise, faster, and less susceptible to errors because of the minimum human interaction compared to many commonly used practices in ophthalmic offices. Minimum human interactions mean less subjective judgments and clearer verdicts on what constitutes a healthy or a glaucomatous eye. The second part of this project analyzes how the optic cup and optic disc are isolated using image processing techniques and algorithms. The last part discusses the results of image processing applied on fundus images to obtain the cup-to-disc ratio.

* 1. PROPOSED ALGORITHM FOR GLAUCOMA DETECTION

# Glaucoma and its Characteristics

Glaucoma is usually linked to a buildup of pressure in the eye caused by fluids, not draining quickly enough through the “angle” as shown in figure 1 [3]. Angle-closure glaucoma is one reason why fluids do not drain. This type of glaucoma occurs when the angle is too narrow and restricts the flow of fluid causing extra pressure on the eye. Similar to angle-closure glaucoma, open-angle glaucoma also builds pressure to the eye but here, the angle is “open” or wide enough to not restrict the flow, yet for unknown reasons, fluids still do not flow through. As fluids build up, they create intraocular pressure in the eye, and tonometry is used to measure this pressure to determine if the eye is glaucomatous. The



*Figure 1: Fluid pathway (in teal) in eye [3]*

device used for this purpose is called a tonometer. It is placed against the eye and measures the pressure. However, according to the National Eye Institute, having an increased eye

pressure does not necessarily mean that a person has glaucoma, as people are different, and some eyes can tolerate higher pressure than others [3].

Having glaucoma depends on how much pressure the optic nerve can handle. This also means that people having low pressure in their eyes could also have glaucoma, which is called low-tension or normal tension glaucoma, a type of the open-angle glaucoma. The pressure that the optic nerve can tolerate is relative and different from one person to another. There is no correct tension threshold to determine if a person has glaucoma. Therefore, the tonometry test is not always accurate.

# Cup-to-disc Ratio


Glaucoma can be determined by calculating the size of the optic disc and the optic cup, the center portion of the optic disc. The optic cup and optic disc are areas in the back of the eye where the retinal nerve fibers are collected to form the optic nerve [10]. According to Kwon, Fingert, and Greenlee [11], the cup is actually “an empty space in the middle of the optic nerve and with the loss of nerve fibers from glaucoma, the cup becomes progressively larger as less space is occupied by the nerve fibers” [11]. The fewer optic fibers an eye has, the bigger the cup becomes, and the ratio of the cup is bigger compared to the disc. A simple representation of the cup-to-disc ratio is shown in figure 2 [11]. In the figure, the optic disc diameter is divided into tenths and the cup is at the center of the optic

4

disc. The cup-to-disc ratio of diameters in figure 2 is then 1#. The area of a circle is 𝐴 =

𝜋𝑟(, where 𝑟 = 𝑑\*𝑎𝑚𝑒𝑡𝑒𝑟. The cup-to-disc ratio in Kwon, Fingert, and Greenlee from figure

(

2 is the diameter ratio, but the cup-to-disc ratio that is discussed throughout the remainder of this project report is the cup-to-disc ratio of areas, which is proportional to the square of the cup-to-disc ratio of diameters.


*Figure 2: Representation of cup-to-disc ratio [11]*

In this project, we used several libraries from MATLAB to implement the proposed methods. MATLAB is matrix-based language that can be used to manipulate and process images through mathematical computations. Its libraries contain many algorithms that can be used to determine the cup-to-disc ratio.



*Figure 3: Fundus photograph [12]*

A fundus photograph (figure 3) is an image describing the inside or back of the eyeball where the optic cup, disc, and blood vessels can be seen. Given a fundus photograph of an eye, the optic disc and cup can be retrieved and isolated and their areas recorded. The optic disc is the brighter circle of the fundus photograph, and the optic cup is the brightest part of the optic disc shown in figure 4. A total of twenty fundus images from Friedrich- Alexander Erlangen-Nuremberg University’s website are used in this project [12].




*Figure 4: Optic disc (in yellow) and optic cup (in green) – cropped from [12]*


# Algorithm Steps

Figures 5 and 6 show the flowcharts of the proposed method for finding the optic disc and cup areas. Figure 5 shows the process of isolating the optic cup. An original fundus image from [12] is adjusted to have a better color contrast between red and yellow. This image is then segmented. At the same time, the red, blue, and green channel histograms are studied to find the threshold that optimizes the transformation of the adjusted superpixeled image into a gray level image. The image is then binarized, and the optic cup is isolated. The optic cup area is then determined using the “regionprops” function. Figure 6 represents the process of isolating the optic disc. The proposed algorithm

finds the optic disc through a loop. First, the red channel is taken from a fundus image and then enhanced. The histogram of this enhanced image is processed to find a threshold. The image is binarized using this threshold, then the algorithm looks for the optic disc. If no optic disc is found, it increases the threshold and binarizes the enhanced image with the new threshold. The algorithm goes through this loop until an optic disc is found or until the threshold is more than 1 on a scale between 0 and 1, in which 1 represents the gray level index of 255. In the case the threshold becomes more than 1, the algorithm does the same process with the blue channel image.



*Figure 5: Find optic cup process*




*Figure 6: Find optic disc process*

* 1. ANALYSIS OF THE DATA

# Healthy vs. Glaucoma Eyes

Figure 7 is a fundus image of a healthy eye, and figure 8 is an image of a glaucomatous eye. Comparing these two images, the brighter yellow area of the optic cup in the glaucomatous image is bigger than the healthy eye. However, the optic cup of the glaucoma eye appears more orange while the optic cup of the healthy eye looks bright yellow. The glaucomatous optic cup’s border and its optic disc’s border do not seem to have a large separation gap between them compared to the healthy eye.



*Figure 7: Healthy eye [12]*

Since the optic cup from the healthy eye is not as big as that of the glaucomatous eye, the healthy eye seems to have a smaller optic disc. The optic cup of the healthy eye seems brighter than the glaucomatous eye’s; it also appears to have more contrast, as the veins are darker and more defined.




*Figure 8: Glaucomatous eye [12]*

# Optic Disc Analysis

In order to determine if a patient has glaucoma, the area of the optic disc needs to be calculated. This means that the optic disc needs to be isolated from the other elements of the fundus image not needed. While it is possible to manually calculate the area, this approach is time consuming and defeats the purpose of having an automated and more precise method. A color image consists of three channels: green, blue, and red. As can be seen in the fundus photograph in figure 3, the dominant color is red. By doing a red channel extraction, the output image representing the red channel is a grayscale image as shown in figure 9, where the value of each pixel is in the range of gray shades from white to black.

A grayscale image has intensity values from 0 to 255, where black is the weakest intensity and white is the strongest. Enhancing the red channel with histogram equalization gives more contrast to the image and hence a better edge definition of the optic cup, shown in the enhanced red channel image from the fundus photograph (figure 10). By comparing the images side by side, the contrast appears more defined in the enhanced red channel

image than in the regular image; the enhanced image has more black pixels and fewer bright pixels than the original red channel image.



*Figure 9: Red channel image from fundus photograph (original figure from [12])*

The function “imhist” is used to get the histogram of the enhanced image in order to find the threshold. The histogram displays the number of pixels of the image for each grayscale intensity. The histogram shows approximately where the brightest pixels are situated on the grayscale index. The histogram of an enhanced red channel image is shown in figure 11. The threshold is determined to be between gray level index 200 and 255, as indexes in this range separate the optic disc from other elements of the fundus photograph, and the optic disc is recognizable as a round shape. If the gray level index is too low, too many pixels are captured, and the optic disc is not well defined. It is then harder to differentiate the optic disc from other elements of the fundus photograph.

The optic disc has the strongest intensity of the gray level image fundus; therefore, its threshold is between level 200 and 255. The initial threshold is chosen as the largest

value of the histogram, the largest number of pixels within this index range. The number of pixels in this range is very high, so there are better possibilities to find the optic disc since the optic disc’s pixel intensities are in this index range, brighter than the rest of the image. The threshold is used to transform the enhanced image to a black and white image as shown in figure 12.




*Figure 10: Enhanced red channel from fundus photograph (original figure from [12])*

The function “imbinarize” converts all pixels above the threshold to white pixels and converts pixels below the threshold to black. At this stage, even if the binarized output image does not show a clear optic disc because the threshold has captured too many white pixels, the algorithm is designed to increase the threshold gradually until an area similar in size to the optic disc is detected.

After transforming the image to binary, any holes within the optic disc are filled using the function “imfill” that fills the image’s different regions’ holes with white pixels. All the data needed are then recorded using function “regionprops”, which measures the

properties of image regions. Centroid, area, perimeter, and major and minor axis length are the properties used from the “regionprops” function in the experiments. The function returns the properties of each image region in the binary image that are used to determine whether or not a region is the optic disc. The function detects many regions as shown in red in figure 13.



*Figure 11: Histogram of enhanced red channel*

An algorithm is then used to filter down all regions to only one as shown in figure

1. For instance, the algorithm consists of determining how circular a region is, comparing the major axis length and the reciprocal minor axis length of each region. If they are close to each other in value, the region would be considered as potential optic disc. The area of the optic disc is also taken into account; the function “regionprops” returns an array of areas which is then sorted from the highest to the lowest. The reason for using descending


order is that after binarizing the grayscale image, some regions consist of only a few pixels; however, the optic disc should be one of the larger areas in the image. Therefore, a descending order allows to detect the optic disc first.



*Figure 12: Binary image of fundus image using threshold (original figure from [12])*


After several attempts to measure the disc’s area from different fundus images, it was determined that the area of the optic disc is between 65,000 and 130,000 pixels, as the optic disc cannot be too small nor too large. For the images used for this project, if the image is projected onto a graph where the origin is the middle of the image, the optic disc’s y-coordinate should always be near the x-axis, that is, close to y = 0, and the x-coordinate could be either close to the left or to the right of the y-axis (figure 15).

If a red circle is found, the function will return the value 1 as an indicator, but if the red circle is not found, it will go through a loop that will gradually increase the threshold until the binary image of the new enhanced image finds only one circle (figure 14). The



*Figure 13: Regions detected by regionprop function (original figure from [12])*


algorithm will stop increasing the threshold when an optic disc-like region is found or when the threshold is more than the maximum gray level value 255.



*Figure 14: Optic disc region detected in red circle (original figure from [12])*

This method does not work for all images, as the quality of the image and the colors can be different depending on the fundus photograph. If a circle is not found from the enhanced red channel due to many pixels with high values outside the optic disc, the next

step is to take the blue channel and its enhanced image. The image itself will be darker, and the optic disc is brighter than the rest of the image; however, the grayscale image could be too dark and the optic disc area smaller.



*Figure 15: Fundus image with optic disc on the left (original figure from [12])*

The same process as for the enhanced red channel image is done with the blue channel. Unfortunately, the method can give less accurate results, as the veins around the optic disc are emphasized. The method may take out the optic disc’s area when the image is transformed into a binary image from the red or blue channel. The strong presence of veins will prevent parts of the optic disc to be seen.

# Optic Cup Analysis

The optic cup is the brightest part of the optic disc; it can be defined as a pallor, a region paler than the rest of the image. However, in some cases, there is no concrete pallor (figure 16) defined in the optic disc, which means that the optic cup is not well defined [8].


To retrieve the optic cup, the red, green, and blue channel histograms of each fundus photograph from the database are analyzed. The optic cup is the brightest region of the fundus photograph, and the color yellow can be compared to the color of the optic cup.



*Figure 16: Example with no distinct optic cup [8]*

A histogram of a color channel represents the distribution of that color in an image. There is no yellow channel to know how many yellow pixels are there. To determine how many yellow pixels there are in the image, the red, green, and blue channel histograms are combined. The number of yellow pixels is where the green channel is in between the red and blue channel histograms, but the red channel histogram curve is above the green channel. However, if there are too many red pixels and not enough green pixels, the image will be orange or redder instead of yellow. An ideal yellow corresponds to having an equal number of green and red pixels. The interception point of the red and green channels is also important, because, if it happens too low in the gray level scale, the image is darker, and the shade of yellow is not as bright.


The study of many histograms reveals that there are two main types of images. In the first type, the red channel clearly intercepts the green channel before gray level index 100, as shown in figure 17. In the second type, the red channel and green channels interception occurs above the gray level index 100 (figure 18).



*Figure 17: Example of green and red channel histograms intercepting before gray level index 100*

The MATLAB “superpixels” function is used to determine the optic cup. This function segments the image into many parts. The “superpixels” function uses a simple linear iterative clustering (SLIC) algorithm that decomposes the image and groups pixels into regions with similar values according to the number of groups the user wants to create [13]. The idea of using “superpixels” is inspired from Jun Cheng’s and his fellow researchers’ paper *Superpixel Classification based Optic Cup Segmentation* [8]. They use classification, smoothing, and ellipse fitting. Depending to the type of image, the number

of pixels for the “superpixels” function may change. The image intensity is first adjusted to make the optic cup more visible compared to the rest of the picture, and then it becomes bright yellow (figure 19).




*Figure 18: Example of green and red channel histograms intercepting after gray level index 100*

The “superpixel” function segments the fundus image according to the level of colors as shown in figure 20. Once the fundus image is segmented, the image is transformed into a grayscale image as shown in figure 21. After several experiments, it is concluded that segmentation of the fundus image into multiple and smaller parts is more efficient in finding the optic cup than segmenting the image into large pieces. The optic cup is the segmented region that has the highest grayscale intensity level, as shown in figure 22.


The binary image of the optic cup can show either a group of pixels or many groups of pixels as the optic cup is traversed by a blood vessel that divides it into many parts. It is

also noticed throughout the experiments on the whole database that white pixels outside of the optic disc are not captured by the “superpixel” method.



*Figure 19: Image adjusted with imadjust function [12]*


The “regionprops” function is then used to determine the area of the optic cup. The




*Figure 20: Image segmented with superpixel function [12]*

area is the sum of all the elements found in the binary image. At this point, both the optic disc and optic cup are found, and the cup-to-disc ratio is now calculated, from which it can

be determined whether or not we have a glaucomatous eye. The results are discussed in the next chapter.



*Figure 21: Gray level superpixel image [12]*



*Figure 22: Binary optic cup isolated [12]*

* 1. FINDINGS AND INTERPRETATIONS

The data in table 1 show the differences between healthy and glaucomatous eyes in terms of the areas of the optic disc and optic cup and the area ratio. The healthy optic disc areas range from 53,572 to 125,736 pixels with an average of 91,585 pixels, while the optic disc areas with glaucoma range from 66,153 to 129,069 pixels with an average of 100,542 pixels. The optic disc area ranges for the healthy eye and glaucoma are not drastically different (the averages differ by less than 10,000 pixels), which shows that the optic disc is not a variable in the cup-to-disc ratio measurement. A healthy optic cup area, according to the data, ranges from 10,352 to 39,011pixels and has an average of 21,519 pixels. With the glaucoma’s optic cup area ranging from 8,576 to 63,206 pixels, the average area of the optic cup for eyes with glaucoma is 30,619 pixels, which is larger than the average area of the optic cup for healthy eyes. The optic cup data for both healthy and glaucomatous eyes have a larger gap; these data indicate that the optic cup area for glaucomatous eye is generally larger than for healthy eyes. However, some optic cup areas from the glaucomatous eyes data are smaller than those for healthy eyes.

For example, in the glaucoma image #1 from table 1, the optic cup is 8,576 pixels which is smaller than any of the optic cups from the healthy and glaucomatous images, and the cup-to-disc ratio is only 0.08. Another extreme case is image #7 of the healthy eye group in which the cup-to-disc ratio is only 0.08; the optic disc is the largest of the fundus photographs, but the cup-to-disc ratio is very small because the optic cup is also very small. The average of the cup-to-disc ratio for the healthy eye data is 0.22, while it is 0.34 for the glaucoma set of data. Image #1 from the glaucomatous eyes data and image #7 from the

healthy eyes data are below average, which indicates that the presence of blood vessels or the quality of the image influenced the data and resulted in a classification error. There are some optic cup areas from the healthy eye group that are larger than for the glaucomatous eye group, such as image #3, in which the area is 39,011 pixels. The data from the table do not correlate well with the known information about glaucoma, which means that some of results are erroneous. There are various reasons behind the errors in the results that will be discussed later.

*Table 1: Glaucoma and healthy optic disc, optic cup sizes (in pixels) and their ratio*





Figure 23 shows the sets of healthy and glaucoma eye data representing the optic cup area as a function of the optic disc area. In the figure, the glaucomatous eyes’ ratio data are grouped together on the far lower right side of the figure, while the healthy eyes’ ratio data incline toward the upper region of the figure. There are some exceptions for some healthy and glaucomatous data that overlap and are found in both the lower and upper

regions of the graph. The overlap of data is caused by the nature of the fundus photographs, such as the presence of extra elements, or by the removal of too much information during the image binarization process. Blood vessels that pass across the optic disc and cup also contribute to reducing accuracy.



*Figure 23: Optic cup area versus optic disc area*

The blood vessels cause the binary optic disc and optic cup to lose some pixels in some areas. For example, in a previous image (figure 14) representing “Optic disc region detected in red circle,” it is shown that the blood vessels are not impacting the area of the optic disc and cup excessively. In some cases, such as in the “Glaucoma’s fundus photograph with heavy blood vessels” (figure 24), the blood vessels hide parts of the optic cup, and optic disc. It can be observed from the “Glaucoma’s optic disc binary image with heavy blood vessels” (figure 25) that the optic disc of the glaucoma eye is not too much

impacted by the blood vessels, but they still have an effect on the optic cup area calculation. In fact, the “superpixels” function cannot detect the brighter part of the optic cup that’s hidden by the blood vessels in this particular view, as it is seen as red and not bright yellow.



*Figure 24: Glaucoma's fundus photograph with heavy blood vessels [12]*

The binary image of the glaucomic eye's optic cup with heavy blood vessels (figure 26) clearly shows how the optic cup is shaped along the blood vessel across it. At one point, blood vessel extraction was considered and attempted following the footsteps of Shahriar Badhsha and his coworkers in *“A New Blood Vessel Extraction Technique Using Edge Enhancement and Object Classification”* [14]. Their method consists of taking the red channel extraction, in which the blood vessels are first enhanced with Kirsch’s template, a set of arrays applied on the image to enhance edges, then the processed image is converted into a grayscale image. The contrasts are then enhanced with the histogram equalization function, and the gray image is converted to binary using Shahriar Badhsha’s threshold.




*Figure 25: Glaucoma's optic disc binary image with heavy blood vessels (original figure from [12])*

Morphological closing, a dual operation that uses dilation to the image followed by erosion, is applied to close the holes and empty areas created by the Kirsch’s template. After several other steps following Badhsha and his collegues’ method, the final output is a binary image of the blood vessel [14]. The blood vessel binary image is used as a mask to remove the blood vessel from the original fundus photograph, but the issue encountered when trying to remove the blood vessels was to apply the binary mask to the RGB image, as applying a binary mask directly to an RGB image is not possible because the images need to be of the same format. If the RGB image is transformed into binary, and the mask is applied, the transformed RGB image loses important information.

Another issue found with some fundus photographs is when the optic cup edges are not well defined. This case prevents the function “superpixels” from getting the correct number of bright yellow pixels. An optic cup with no defined pallor blends into the optic disc and looks like it does not exist; therefore, the “superpixels” function will give either a


very large area, as the brightest pixels are not as visible, and pixels from the optic disc will be captured as the brightest pixels, resulting in bigger area, or a very small area, as only a few pixels in the middle of the optic cup are detected. For instance, a healthy fundus photograph with no optic cup (figure 27) and the binary image of a healthy optic disc (figure 28) demonstrate the effect of “no distinct optic cup.” The presence of blood vessels affects the calculation of the area as well, but it does not impact it drastically. The over- segmented fundus photograph of the healthy eye shows that the brighter area is not the center of the optic disc (figure 29).



*Figure 26: Glaucoma's optic cup binary image with heavy blood vessels (original figure from [12])*

As there is no defined pallor in the fundus photograph, the brighter yellow area is in this case expanded outside of the supposed optic cup area. The binary image of the healthy over-segmented fundus photograph from figure 29 displays the optic cup differently from how it is supposed to look and where it is supposed to be to the naked eye in comparison to the original image from figure 27. In this case, the optic cup is not in the


center of the optic disc; instead the optic cup is located in the optic disc’s left side area. As explained previously, when no optic cup is defined, it is more difficult to over-segment the image.



*Figure 27: Healthy fundus photograph with no defined optic cup [12]*


One idea to address the issue is to examine whether a fundus photograph has a distinct pallor. If it does not, then it is possible get the actual status of the patient eye (whether the eye is glaucomatous or healthy) and make a learning algorithm that is able to give more accurate results for each image with no pallor. The next steps are the same as adjusting and over-segmenting the image, but instead of using the same number as the fundus image with pallor, the image should be over-segmented two to three times more in order to get smaller groups of pixels that can be classified by their intensity and positions. By superposing the original fundus photograph with the over-segmented image, an approximation of the optic cup area can be made. A relationship between glaucoma and healthy eyes can be linked with the fundus images with no pallor, keeping a record of each

image and reusing them in the next fundus with no defined pallor to analyze. The algorithm



*Figure 28: Binary image of healthy eye with no distinct cup (original figure from [12])*

can learn and add data each time it analyzes a fundus photograph of this category. The method described above would be interesting to develop but very costly, as well, because it would be time consuming for the “superpixels” function to just over-segment the fundus photograph into that many groups of pixels. The current number of pieces required to



*Figure 29: Healthy optic cup extraction - no defined optic cup case (original figure from [12])*

divide the image in this project already makes the process slow, so using twice as much segmentations would not be reasonable unless the machine running process is faster.

All fundus images studied here were 2D images. With today’s technology, 3D fundus images are possible to acquire, such as the image shown in figure 30 [13]. Doctors are able to get a 3D image of the eye fundus easily. As can be seen in figure 30, the image is clearer, and the optic disc is not distorted. When comparing 2D and 3D images, 2D images have their optic cup slightly oval, while in 3D images, the optic cup is more circular. The colors are also different, and 3D images have more contrast, which could make it easier to obtain the optic cup and disc. The algorithms used on 2D images would also work on 3D images, as the fundamental properties are the same. As 3D imaging technology advances, it will be easier to detect glaucoma in the future.



*Figure 30: 3D Fundus photograph [15]*

* 1. SUMMARY AND CONCLUSIONS

Glaucoma, thief of sight, is an eye disease touching millions of people. If not treated in a timely manner, it can result in permanent vision loss. There are several methods to detect glaucoma. One traditional method is by measuring the patient’s eye pressure. The higher the eye pressure is, the more likely the patient is to have glaucoma. However, eye pressure can be subjective, because how much pressure an eye can handle depends on the person; some people’s optic nerves are more sensitive to pressure than others. A person can have a high eye pressure without having glaucoma, while another can have glaucoma with lower eye pressure. This condition is called low pressure glaucoma.

Instead of measuring eye pressure, the eye’s optic cup-to-disc ratio is measured. By measuring the optic cup-to-disc ratio on a fundus photograph, it is possible to determine if a person has glaucoma. The cup is an empty space in the middle of the optic nerve; when damaged, the optic nerve deteriorates and atrophies, making the optic cup bigger, which results in a larger cup-to-disc ratio. The more damaged the nerves are, the bigger the optic cup is. Computational and image processing techniques can play an important role in solving the problem. Many researchers are developing better techniques to identifying glaucoma through image processing.

In this project, different methods were used to first get the optic disc and optic cup. The goal is to use the enhanced red channel image, find the threshold, and use it to binarize the image. The output image is then analyzed to determine the optic disc’s location. Characteristics such as the size and position on the image are keys to determine which elements make up the optic disc. If no circle is found, this process goes through a loop,

increasing the threshold until one circle is found. If no circle is found, the blue channel is used instead of the red channel. The optic cup is found by intensifying the brighter color of the image (which is the optic cup) and by using the “superpixel” function that segments the image into pieces. The picture is then transformed into a grayscale picture, and the threshold which is the index of the brightest segmentation is used to transform the image into binary. The cup-to-disc ratio is then calculated.

The results show that glaucomatous eyes, on average, have a bigger cup-to-disc ratio than healthy eyes. Some results were not as expected, such as healthy eyes being detected as glaucomatous eyes by having a larger cup-to-disc ratio and some glaucomatous eyes being detected as healthy eyes by having a smaller cup-to-disc ratio. This can be explained by the heavy presence of blood vessels across the optic disc and cup in some cases, and non-obvious presence of optic cup definition when no pallor is detected. A step that can be added to the algorithm to make it more accurate is by extracting the blood vessels along with the reconstitution of the empty area. Another step is also to detect when a fundus photograph does not have an obvious pallor for the optic cup. It is proposed to train a learning algorithm to recognize when no pallor is clearly detected, and in this case, not attempt to classify whether the eye is glaucomatous or not, instead of giving false positive or negative results.

Glaucoma disease can be detected from a 2D fundus photograph but also 3D imaging can be used. In fact, 3D fundus imaging is emerging, and doctors are now able to take a 3D fundus photograph in one take [15]. This could help in recognizing glaucoma and other diseases at the same time more easily. Cameras are getting better and provide

excellent images. The proposed methods can use a 3D fundus photograph, as the 3D photograph is laid out as a 2D panoramic view of the entire eye with better contrast of colors.

Works Cited

1. Glaucoma Research Foundation, "Glaucoma Facts and Stats," Glaucoma Research Foundation, 18 November 2016. [Online]. Available: [http://www.glaucoma.org/glaucoma/glaucoma-facts-and-stats.php.](http://www.glaucoma.org/glaucoma/glaucoma-facts-and-stats.php) [Accessed 10 February 2017].
2. Glaucoma Research Foundation, "Types of Glaucoma," Glaucoma Research Foundation, 18 August 2016. [Online]. Available: [http://www.glaucoma.org/glaucoma/types-of-glaucoma.php.](http://www.glaucoma.org/glaucoma/types-of-glaucoma.php) [Accessed 11 February 2017].
3. National Eye Institute, "Facts About Glaucoma," National Eye Institute, [Online]. Available: https://nei.nih.gov/health/glaucoma/glaucoma\_facts. [Accessed 23 01 2017].
4. M. Yvonne Ou, "Is Glaucoma Painful?," Bright Focus Foundation, 24 May 2017. [Online]. Available: <http://www.brightfocus.org/glaucoma/article/glaucoma-> painful. [Accessed 1 June 2017].
5. Glaucoma Research Foundation, "What are the Symptoms of Glaucoma," Glaucoma Research Foundation, 10 May 2017. [Online]. Available: [http://www.glaucoma.org/gleams/what-are-the-symptoms-of-glaucoma.php.](http://www.glaucoma.org/gleams/what-are-the-symptoms-of-glaucoma.php) [Accessed 17 May 2017].
6. M. M. Kawde and V. K. Bairagi, "Early Detection of Glaucoma using Image Processing," *Indian Journal of Science and Techbology,* vol. 9 (30), August 2016.
7. Glaucoma Research Foundation, "Five Common Glaucoma Tests," 22 April 2013. [Online]. Available: <http://www.glaucoma.org/glaucoma/diagnostic-> tests.php. [Accessed 13 June 2017].
8. J. Cheng, J. Liu, D. Tao, F. Yin, D. W. K. Wong, Y. Xu and T. Y. Wong, "Superpixel Classification Based Optic Disc and Optic Cup Segmentation for Glaucoma Screening," *IEEE Transactions on Medical Imaging,* vol. 32, no. 6, pp. 1019-1032, June 2013.
9. M. Madhusudhan, N. Malay, S. Nirmala and D. Samerendra, "Image Processing Techniques for Glaucoma Detection," *Communications in Computer and Information Science,* pp. 365-373, July 2011.
10. Glaucoma Research Foundation, "Optic nerve cupping," 21 August 2012. [Online]. Available: <http://www.glaucoma.org/treatment/optic-nerve-> cupping.php. [Accessed 10 February 2017].
11. Y. H. M. P. Kwon, J. H. M. P. Fingert and E. C. M. P. Greenlee, "A Patient's Guide to Glaucoma: Section 1-B. The Meaning of Cupping," 27 February 2006. [Online]. Available: <http://www.medrounds.org/glaucoma-> guide/2006/02/section-1-b-meaning-of-cupping.html. [Accessed 5 February 2017].
12. Friedrich-Alexander-Universität Erlangen-Nürnberg, "High-Resolution Fundus (HRF) Image Database," [Online]. Available: https://www5.cs.fau.de/research/data/fundus-images/. [Accessed 20 February 2017].
13. MathWorks, "2-D Superpixel Oversegmentation of Image - MATLAB Superpixels," [Online]. Available: https://[www.mathworks.com/help/images/ref/superpixels.html.](http://www.mathworks.com/help/images/ref/superpixels.html) [Accessed 13 04 2017].
14. S. Badsha, A. W. Reza, K. G. Tan and K. Dimyati, "A New Blood Vessel Extraction Technique Using Edge Enhancement and Object Classification," *Journal of Digital Imaging - The Journam of the Society for Computer Applications in Radiology,* vol. 26, no. 6, pp. 1107-1115, 2013.
15. R. Rajecki, "Retinal Camera Produces 3D Stereo Images in One Shot," Optometry Times, 01 April 2011. [Online]. Available: <http://optometrytimes.modernmedicine.com/optometrytimes/news/modernmedici> ne/modern-medicine-feature-articles/retinal-camera-produces-3d-stere?page=full. [Accessed 24 May 2017].